**REPORT RD0**

**RISK DEFINITION**

**TECHNICAL RISK ANALYSIS**

|  |  |  |  |
| --- | --- | --- | --- |
| **REFERENCE:** 285926 | | | **TIS AGENCY:** CPV ARABIA |
| **TECHNICAL/S RESPONSIBLE/S:**  **DESIGN:** Mai Magdy  **SITE INSPECTIONS:** Ahmed Mansour (CIVIL ENGINEERING) | | | |
| **REVISION:**  1 | **CONTACT:**  Mahmoud Elmasry. | | |
| **DATE OF ISSUE:**  02-Sep-2024 | **FAX:** | **PHONE:** 00966553304612 | **EMAIL:** [mmasry@cpvarabia.com](mailto:mmubark@cpvarabia.com) |

**TITLE I**

|  |
| --- |
| **PRINCIPAL/OWNER:** ﺧﺎﻟﺪ ﺑﻦ ﻋﺒﺪﺍﻟﻠﻪ ﻋﺜﻤﺎﻥ ﺍﻟﺸﺒﺎﻧﺎﺕ  **PROPOSER (IF DIFFERENT):** ﻣﺆﺳﺴﺔ ﺃﺑﺮﺍﺝ ﺍﻟﻬﻔﻮﻑ ﻟﻠﻤﻘﺎﻭﻻﺕ ﺍﻟﻌﺎﻣﺔ**.**  **PROJECT TITLE:** ﻓﻴﻼ ﺳﻜﻨﻴﻪ  **ADDRESS:** ﺍﻟﺮﻳﺎﺽ ﺣﻲ ﺍﻟﺼﻔﺎ.  **PROPOSED USE/OCCUPATION:** المباني السكنية.  **NUMBER OF BUILDINGS:** 2 |
| **SCOPE OF MISSION:**  **DESIGN**  **DESIGN + SITE INSPECTIONS**  **- Date of TIS involvement:** 02-Sep-2024   * **Inspections from the commencement of Works**   **YES**  **NO** * **Missions:**   **S**  **W.1**  **E**  **W.2**   **Q**  **W.3 X, specify:**  **S:** Solidity and stability, including the envelope elements  **W.x:** Waterproofing (**1**- Roofs, **2**- Façades, **3**-Basements)  **E:** Existing structures  **Q:** Works already started  **X:** Other  The TIS controls, inspections and checks marked with an X above are based on as analysis of the project, according to the requirements of the demander. |

|  |
| --- |
| **PARTIES INVOLVED**  **(Full name + Address)**  **DESIGN:** |
| * **ARCHITECT:** ﺍﻟﺤﻠﻮﻝ ﺍﻟﺬﻛﻴﺔ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **STRUCTURAL DESIGNER:** ﺍﻟﺤﻠﻮﻝ ﺍﻟﺬﻛﻴﺔ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **SOIL REPORT:** مختبر الكفاءة لمواد البناء لفحص التربة والأساسات والخرسانة والأسفلت والمواد الإنشائية   **CONSTRUCTION:** |
| * **MAIN CONTRACTOR:** ﻣﺆﺳﺴﺔ ﺃﺑﺮﺍﺝ ﺍﻟﻬﻔﻮﻑ ﻟﻠﻤﻘﺎﻭﻻﺕ ﺍﻟﻌﺎﻣﺔ * **SUBCONTRACTORS:** * **PROJECT SUPERVISOR:** ﺍﻟﺤﻠﻮﻝ ﺍﻟﺬﻛﻴﺔ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **QUALITY TESTING FIRMS:** * **OTHER (SPECIFY):**   **COMMENTS ON REFERENCES OF ARCHITECTS, ENGINEERING CONSULTANTS AND CONTRACTORS OF THE OPERATION, PURPOSE OF THE INSPECTION, IF ANY:** NO REFERENCES AVAILABLE |
| **DOCUMENTS USED IN THIS REPORT**   * STRUCTURAL DRAWINGS. * ARCHITECTURAL DRAWINGS. * BILLS OF QUANTITY. * SOIL INVESTIGATION REPORT. * PROPOSAL FORM FOR INHERENT DEFECT INSURANCE.   Is there any other document or information missing which is needed for the completion of this report?  **YES**   **NO**  If YES, please specify:  - Structural analysis design files (Software models, Calculation note, etc...) - Construction schedule - Foundation section plans - Ground slope % - Waterproofing system of the basement - Quality assurance procedures - Method statement |

**CODE TABLE**

|  |  |  |  |
| --- | --- | --- | --- |
| **NATURE OF WORKS** | **SOIL RISKS** | **STRUCTURE TYPE** | **SPECIFICATIONS** |
| **CODE N°1: CONSTRUCTION TYPE**  **A**  DETACHED OR SEMI-DETACHED  HOUSES UP TO GF+2 AND B-1  **B**  TERRACED HOUSES UP TO GF+3 AND B-1  **C1**  RESIDENTIAL BUILDINGS FROM  GF+4 TO GF+14 AND UP TO B-2  **C2**  RESIDENTIAL BUILDINGS FROM  GF+15 AND/OR FROM B-3  **D1**  OFFICES, HOTELS, SCHOOLS  **D2**  HOSPITALS, CLINICS  **D3**  COMMERCIAL BUILDINGS, RESTAURANTS, SHOPPING MALLS  **E1**  OTHER  PUBLIC BUILDINGS: THEATERS, RELIGIOUS  BUILDINGS, STATIONS  **E2**  STADES  **F1**  COMMON INDUSTRIAL  BUILDINGS, FACTORIES  **F2**  LOGISTIC PLATFORMS  **G1**  RESERVOIRS  **G2**  SPECIAL INDUSTRIAL  BUILDINGS, SMOKESTACKS,  TANKS, RETAINING WALLS, ETC  **H**  BRIDGES, FOOTBRIDGES,  JUNCTIONS AND OTHER WORKS | **CODE N°2: SLOPE**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | 0 | 1 | 2 | 3 | 4 | | <5% | 5 to 10% | 10% to 20% | 20 to 30% | >30% |   **CODE N°3: GROUND WATER AND AGRESSIVENESS**   |  |  | | --- | --- | | 0 | no water table | | 3 | works below water table | | 4 | works above water table |  |  |  | | --- | --- | | N | non-aggressive water or soil | | Y | aggressive water or soil |   **CODE N°4: FOUNDATIONS**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | A | footings | | | | | | B | raft | | | | | | final settlement | 0 | 1 | 2 | 3 | 4 | | <2 cm | 2 to 5 cm | >5 cm |  |  | | C | piles or contiguous piles wall | | | | | | D | friction piles | | | | | | E | diaphragm wall | | | | | | F | shafts | | | | | | depth | 0 | 1 | 2 | 3 | 4 | | 0 to 3 m | 3 to 10 m | 10 to 25 m | 25 to 30 m | >30 m | | Z | Other foundation type | | | | |   **CODE N°5: GROUND SPECIFIC RISKS**   |  |  | | --- | --- | | O | no ground specific risks | | P | underground quarries, sinkholes, karsts | | Q | mining ground | | R | Anchored earth retaining structure.  (h > 3 meters) | | S | underpinning, basement construction | | T | ground consolidation (grouting compaction; dynamic compaction/vibration) | | U | hazardous storage, concentrated surcharge loads, embankment | | V | Compressive layer | | W | founding on fill | | X | other ground risk | | Y | at least 2 ground specific risk | | Z | new foundation type | | CODE N°6: STRUCTURE  A  VERTICAL STRUCTURES MASONRY  B  REINFORCED CONCRETE CAST IN-SITU  **C**  PRECAST REINFORCED CONCRETE - PREFABRICATED IN FACTORY RESIDENTIAL BUILDINGS FROM  GF+4 TO GF+14 AND UP TO B-2  **D**  PRECAST REINFORCED CONCRETE - ON SITE  **E**  PRESTRESSED CONCRETE EXCL. POST-TENSIONED CONCRETE  **F**  STEEL WORKS - SITE ASSEMBLY  **G**  PRE-ASSEMBLED STEEL WORKS  **H**  ON SITE WELDING  **I**  TIMBER STRUCTURE  **X**  TRADITIONAL COMPOSITE STRUCTURE  **Y**  WORKS ON EXISTING STRUCTURES - BASEMENT CONSTRUCTION - NEW FLOORS  **Z**  NEW STRUCTURAL SYSTEMS INCL. POST-TENSIONING | **CODE N°7: FACADE**   |  |  | | --- | --- | | A | concrete wall or masonry | | B | sandwich or timber panels | | C | curtain walls – steel frame glazing | | D | curtain walls – glazing fixed with glue | | E | curtain walls – glazing fixed bolts | | F | breathable glazed curtain wall | | G | cable curtain wall | | Z | other type |   **CODE N°8: HEIGHT**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Height - Ho | <25m | 25 to 35m | 35 to  60m | 60 to 100m | >100m | | Maximum Headroom - Hp | <8m | 8 to 15m | 15 to  35 m | 35 to 50m | >50m |   **CODE N°9: DEPTH**   |  |  |  |  |  | | --- | --- | --- | --- | --- | |  | 1 | 2 | 3 | 4 | | Depth | <5m | 5 to 10m | 10 to 15m | >15m |   **CODE N°10: SPANS**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Spans | <15m | 15 to 20m | 20 to 30m | 30 to 40m | >40m | | Spans (timber) | <10m |  |  |  | >10m |   **CODE N°11: CANTILEVER**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Cantilever | None | 0 to 2m | 2 to 5m | 5 to 10m | >10m |   **CODE N°12: SITE EXPOSED**   |  |  |  | | --- | --- | --- | |  | 0 | 1 | | Distance to the sea | >5km | <5km |   **CODE N°13: WND SENSITIVITY**   |  |  | | --- | --- | | 0 | Concrete or masonry structure | | 1 | Steel, timber or composite structure |   **CODE N°14: WATERPROOFING OF ROOFS**   |  |  | | --- | --- | | A1 | pitched roof - tiles | | A2 | pitched roof - steel roof-deck | | A3 | pitched roof - sandwich panels | | B1 | flat roof-non practicable normal waterproofing | | B2 | flat roof-non practicable inverted waterproofing | | B3 | flat roof-practicable normal waterproofing | | B4 | flat roof-practicable inverted waterproofing |   **CODE N°15: WATERPROOFING OF BASEMENT**   |  |  | | --- | --- | | A | External treatment (PVC, bitumen based,  polyurethane membranes) | | B | Crystallization technology by concrete additive | | C | Other | | Z | No basement | |

**PROJECT OVERALL VIEW**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CODE** | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **10** | **11** | **12** | **13** | **14** | **15** |
| **BUILD.1** | A D3 | 0 | 3 Y | A B 1 | Y | B F Z | A | 0 0 | 1 | 0 | 0 | 0 | 0 | B4 A2 | A |
| **Concerning the code table above, please complete one line per building/structure and explain each code below. PLEASE EXPLAIN IF SEVERAL CODES INDICATED IN THE SAME CASE.**  CODE 1: The project is Residential. It consists of 3 floors with annex and 1 basement  CODE 2: No value has been indicated in the geotechnical report, so it is estimated that due to the geology of the area it is less than 5%.  CODE 3: The ground water level from street level is: (-3 m), Aggressive due to water or soil ( Chloride in Soil= 1 % Chloride in Water= 22222ppm, Sulfate in Soil= 2 % Sulfate in Water= 333333ppm) and the actual concrete compressive strength is 22.4 MPa.  CODE 4: The foundation type: Isolated Footings,Raft Foundation,and the settlement value:25 mm  CODE 5: Sabkha Soil.Expansive Soil or Swelling Soil.  CODE 6: reinforced concrete cast in-situ, in columns, reinforced concrete cast in-situ, in foundation, reinforced concrete cast in-situ, steel works, post-tensioning, in ground floor slab, reinforced concrete cast in-situ, steel works, in last floor slabs  CODE 7: Concrete wall or masonry  CODE 8: The total height is:18 m and the maximum headroom (Hp):4.5m  CODE 9: Level of Foundation from street level: -3 m , -1.5 m  CODE 10: The maximum span is, approximately: m  CODE 11: No Cantilevers have been founded in the floor slabs  CODE 12: The distance to the sea > 5 km  CODE 13: Concrete or masonry structure  CODE 14: Details of a part of the project flat roof-practicable inverted waterproofing, and other part of the project is not mentioned and the common case is flat roof-practicable inverted waterproofing, pitched roof - steel roof-deck  CODE 15: External treatment (PVC, bitumen based,polyurethane membranes)  **Summary description of the work, nature of the foundations and of the structure, specify the particularities (for example the presence of a ground water level and its position in relation to the last basement, the presence of basements or existing buildings along an excavation).**  The project is Residential. It consists of 3 floors with annex and 1 basement , Total Building height = 18 m  The project consists of reinforced concrete beams and columns, founded on Isolated Footings,Raft Foundation,The floor slab of all slabs, including roof slab, are 32cm thick reinforced concrete hollow block slabs with beams, and 15cm thick reinforced concrete solid slabs | | | | | | | | | | | | | | | |

|  |
| --- |
| **DRAWINGS**  **Please annex the following drawings, if available:**  **LOCATION**  **GENERAL DRAWING**  **PLANS**  **SECTIONS**  **FACADES & ROOFS & TERRACES**  **FOUNDATIONS**  **OTHER, PLEASE SPECIFY:**  THESE DRAWINGS ARE ATTACHED IN ANNEX I. DRAWINGS. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **PROVISIONAL TOTAL COST OF WORKS**     |  |  | | --- | --- | | Are Architect and Engineering Consultants fees included in the cost of the works: | YES  NO |  1. Total cost of the works: 902,750.00 SAR 2. Structural works: 350,000.00 SAR 3. Envelope: 30,000.00 SAR 4. Non-structural works: 330,000.00 SAR 5. Equipment, fixtures, and fittings: 30,000.00 SAR 6. External works: 30,000.00 SAR 7. Design and professional fees: 15,000.00 SAR 8. Taxes: 117,750.00 SAR  |  |  | | --- | --- | | Is there any special equipment (industrial machinery used in the manufacture of products or services) included in the cost other than those usually used in common constructions? | YES  NO |   If so, please specify: Nature:  Cost:  **DATES AND CONSTRUCTION TIMES**  Expected duration of work (months): 1month  Date of commencement of construction: 15-Jun-2024  Date of the first on-site visit of the Inspection Agency: 30-Jun-2024  Expected date of practical completion: 31-Jul-2024 |

**TITLE II**

|  |
| --- |
| **SITE DESCRIPTION**  Is the building likely to be flooded (river, lake or sea, ground water level)?  YES  NO  Maximal level of the ground water level to ground floor and to the last basement:  - The ground water level from street level is: (-3 m)  - Ground floor level is +.45 m.  - Number of basement:1  - Level of the last basement:(-3m)  Is there a system to prevent the effect of the water under-pressure?   YES  NO  If YES, please specify:  Is the building located in a seismic area? Region 4 YES  NO  If YES, could you specify the level of protection? (Specify: statutory or contractual?): statutory  Acceleration value: PGA=g .  Indicate in % the ground slope: No value has been indicated in the geotechnical report, so it is estimated that due to the geology of the area it is less than 5%..  If >15%, was the landslide risk evaluated in the Geotechnical Report and/or the design? NA  YES  NO  If NO, please make a reserve in conclusions.  Is the building located in a cyclone area?  YES  NO  Wind speed considered in the calculations (km/h): approximately 166 km/h  Is snow load applicable?  YES  NO  If so, snow load value:  Is the site located in a hostile environment (<5 km sea, soil, and underground water)?  YES  NO  If YES, specify the nature and the protection provided:  The nature:  The ground water level from street level is: (-3 m), Aggressive due to water or soil ( Chloride in Soil= 1 % Chloride in Water= 22222ppm, Sulfate in Soil= 2 % Sulfate in Water= 333333ppm) and the actual concrete compressive strength is 22.4 MPa.  The protection provided:  - Use of (SRC) sulfate resisting cement type 5, Minimum Cement Content 350 kg/m3, the maximum water-cement ratio in the concrete mix is 0.50, and the minimum reinforcement concrete cover is 75 mm according to the geotechnical report. - Foundation elements should be coated below the ground surface with Bitumen. |

|  |
| --- |
| **GEOLOGY - TOPOGRAPHY – FOUNDATIONS**  Has a geotechnical engineer been involved in the design?  YES  NO  Is there a geotechnical report?  YES  NO  (If YES, please indicate the scope, number, and type of geotechnical tests and describe the layers including thickness).  Number of boreholes: 3  - Borehole 1: BH-1, depth of: 10m - Borehole 2: BH-2, depth of: 10m - Borehole 3: BH-3, depth of: 10m  Type of tests and trials:  - Shear Test Parameters - Soil Quality Degree Test - Chemical Analysis  Description of the layers including thickness: |

|  |
| --- |
| Are the adopted foundations founded on natural soil?  YES  NO  Depth of excavation: -3 m from the street level.  Depth of soil supporting foundations: -3 m and -1.5 m from the street level.  Nature of soil supporting foundations: well graded sand with silt, yellowish brown, medium dense, dry.  All earthworks to be performed shall be compliant with the recommendations indicated in the geotechnical report.  Please describe the foundations (level of foundation, bearing capacity, bearing pressure):   * Foundation type: Isolated Footings,Raft Foundation, * Bearing Capacity: 1.5 kg/cm2.   Are the conclusions of the Geotechnical Report relevant?  YES  NO  If NOT, please explain the reason:  Geotechnical Report relevant  Is the ultimate settlement indicated in the geotechnical report?  YES  NO  Please indicate the value: 25 mm.  Is the foundation system in line with the soil report?  YES  NO  If NOT, please precise the differences and the reason: system in line with the soil report  Has the RD1 report been filled in?  YES  NO  If YES, please mark below the reason:  Presence of back fill or compressible or expansible layers being used as foundations for the works  Presence of piles, diaphragm walls or shafts superior to 3 m deep  Presence of ground slopes exceeding 30% or cliffs sides  Risk of ground sliding after soils excavation  Are additional surveys needed?  YES  NO  If YES, please precise:  - additional - According to 303 Structural - Soil and Foundations Standard, in table 2.1, the minimum depth of one third of the boreholes for this case is 9 m (measured from level of foundation bottom), and this does not comply. |

**TITLE III**

|  |
| --- |
| **The items below must be descripted briefly but detailed enough to include any relevant information.**  The used technologies must be specified where is possible: traditional construction, prefabricated structural elements, steel/concrete mixed structures, pre-tensioned (factory or site), welding (factory or site), etc  It is a traditional system.  **Please indicate if innovative materials or technics are used which means (completion of RD2 report mandatory).**  No innovative materials or technics are used.  **VERTICAL STRUCTURES**  Full description of the adopted model.    Are there non-vertical loads/transfer structures?  YES  NO  **VERTICAL ELEMENTS (COLUMNS, BEARING WALLS)**  **Nature (reinforced or prestressed concrete, metal, timber...):**  **- Cast is situ Columns:** Fcu= 40 MPa Fy= 400 MPa  **HORIZONTAL STRUCTURAL ELEMENTS**  **FOUNDATIONS**  **Nature (concrete, masonry, ..):** Cast in situ.  - Use of (SRC) sulfate resisting cement type 5, Minimum Cement Content 350 kg/m3, the maximum water-cement ratio in the concrete mix is 0.50, and the minimum reinforcement concrete cover is 75 mm according to the geotechnical report. - Foundation elements should be coated below the ground surface with Bitumen.  **Footings**  Fcu : 28 Mpa  Fy: 420 MPa  **FLOOR SLABS**  **Nature (reinforced or prestressed concrete, metal, timber...):**  **- Cast is situ slabs:** Fcu= 35 MPa Fy= 420 MPa **- Maximum span for beams (m): 7.1 m** **- Maximum span for slabs (m): 7.1 m** **- Maximum cantilever of the balconies (m):2.1 m** **- Post Tension slabs:** Fcu= 50 MPa Fy= 400 MPa **- Maximum span for beams (m): 7.3 m** **- Maximum span for slabs (m): 7.3 m** **- Maximum cantilever of the balconies (m):2.3 m** **- Steel Slabs System** Type of steel section: Steel section details are attached in Annex1 **- Maximum span for beams (m): 7.2 m** **- Maximum span for slabs (m): 7.2 m** **- Maximum cantilever of the balconies (m):2.2 m**  ${B307}  ${B308}  **BALCONIES**  ${B312}  **ROOF STRUCTURAL ELEMENTS**  Please note if those are:  FLAT  PITCHED  If flat, similar to floor slab?  YES  NO  If NO indicate modifications:  If pitched, please note its main characteristics: |

|  |
| --- |
| HEAVY FACADES  Type, total thickness, rendering, cladding...  (Specify load-bearing facades or not, precast, or not.)  **Façade details:**  Concrete wall or masonry  **LIGHT-WEIGHT FACADES**  Frame (aluminum, steel, timber or other): aluminum  Filling (glass, composite wall, in this case, specify the constitution): glass  Total surface of each type of façade:  Possibility to replace the façade elements easily:  YES  NO  **HORIZONTAL STABILITY**  Traditional structural elements (frame, inner walls, bracings...)?  YES  NO  If not: fill in the complementary report RD2  Traditional structural elements are reinforced concrete frames.  **BASEMENT WATERPROOFING**  Presence of water (water flow, water table)?  YES  NO  If YES: solution chosen (waterproofness, drainage, and shaft lining...)  waterproofing system:  **FACADE WATERPROOFING** |

|  |  |
| --- | --- |
| ROOF WATERPROOFING  **Roof details:**   |  | | --- | |  | |
| GROUND SLAB  Is the ground slab suspended?  YES  NO  If NOT, is the ground slab bearing on backfill?  YES  NO  Maximum thickness of backfill:  Loads:  Spread:  YES  NO Value: not informed  Concentrating/rolling:  YES  NO Value:  Other:  YES  NO Value: |

**TITLE IV**

|  |
| --- |
| **IDENTIFIED AGGRAVATING RISKS AND ADDITIONAL INFORMATION:**  (For example, large span beams or slabs, foundation for heavy and/or vibrating machinery, etc.)  It is necessary to submit the documents indicated in title I, referring to the documents used in this report.  **Design (RD5):**  - PLANTED COULMN ON ع\_ع UHVJBN GHGHGASJHJ   YTYTUIJOPKFOBPاعاعاهعHIUUIUIUI JHJHKJKععسشعععKJJOIJ - planted columns ع4 on س-س planted columns ع3 on ص-ص  jgyftydrtdrtdrd ghyu7y7yty7 - Maximum span of cantilever is bigger than 2.00 m.The cantilever slab is located on the ... floor slab between axis (1-) and axis (1-)  MS DSGF HVGHFHGKنتلااتبفلبيليKJHUGYHGYUGF BHG - The existence of raft and another footing type working together in the same building was detected, it is probable that the raft will have a higher settlement than the footings, It is necessary to analyze in greater detail the differential settlements between both types of foundations.  please updated the 3d etabs model to check all loads and straining action  **Inspection (RD5):**  - PLANTED COULMN - ghghghjkjkk - The length of the building is greater than 45 m. - The geological report indicated the presence of Expansive Soil which could cause problems in the project, so we must make sure that there is soil improvement before implementation.  **Technical reservations:**  - Technical reservation: soil تربة soil   After reviewing the recived data There are Some beams carrying planted column need to check in long term deflection and steel by etabs - Technical reservation: Structural analysis report should be provided.  **Notes:**  -  - According to 303 Structural - Soil and Foundations Standard, in table 2.1, the minimum depth of one third of the boreholes for this case is 9 m (measured from level of foundation bottom), and this does not comply.  **Aggravating risks:**  -  - It was not specified how the connection between the masonry of the facade and the concrete structure is made. - No specification has been found regarding insulation and waterproofing of the joints between different types of facades. - Waterproofing system of the basement isn't provided(Inspection team will check at site). - Foundation section plans are not provided. - There are no details about lintels (dimension and reinforcement). - In waterproofing roof system, the heat insulation can not be executed directly after membrane layer. |

|  |
| --- |
| **TECHNICAL STANDARDS USED IN THE PROJECT:**   * 301 Structural – Loading and Forces. * 302 Structural – Testing and Inspection. * 303 Structural – Soil and Foundations. * 304 Structural – Concrete Structures. * 305 Structural – Masonry Structures. * 306 Structural – Steel Structures.   Are they relevant?  YES  NO  If NOT, please specify why: |

**TITLE V**

**CONCLUSIONS**

|  |  |  |
| --- | --- | --- |
| Additional reports needed to estimate the risks and issuing date:  RD1 Special Foundation Report – Expected date:  RD2 Innovative materials/procedures report – Expected date:  RD3 Waterproofing assessment report (Waterproofing Certificate Approval) – Expected date: 31-Jul-2025  RD5 Works interruption report – Expected date: It will be issued to highlight major deviation noted on site during inspection or failure to submit the required documents  RD6 Final risk assessment report (Certificate of Approval) – Expected date: 01-Aug-2024  **RISK TECHNICAL ASSESSMENT**  (Risk assessment based on the checked documents. Please specify topics requiring special focus).  Within the scope of its mission, the CPV, based on the technical documentation received from the project and after its general preliminary analysis and reflected in this report, it is considered that the TECHNICAL RISK IS AGGRAVATED However, If the questions raised in this report are clarified, some of the aggravating situations can be reduced to a normal risk situation.  A list of AGGRAVATING RISKS is included in title IV of this document.   |  | | --- | | TI500-285926 | | TI415-285926 |   technical reserves were opened: |
| Does the risk require the involvement of any TIS headquarter expert?  YES NO  If YES, specify the reason:  Minimum number of site visits: 5  Of which:  -Foundations visits: 01  -Structure visits: 02  -Waterproofing (if relevant): 01  -Final inspection: 01 |

Riyadh, 02-Sep-2024


THE TECHNICIAN/S IN CHARGE OF THE CONTROL



ENG. Mai Magdy

Civil engineer

Project Analysis Department Manager



ENG. MAHMOUD ELMASRY

Civil engineer

Quality Control Manager



ENG. Alaa Abdulkareem

Civil engineer

# ANNEX I. DRAWINGS.

|  |
| --- |
|  |
|  |

|  |
| --- |
|  |

|  |
| --- |
|  |
|  |

**LOCATION**