**REPORT RD0**

**RISK DEFINITION**

**TECHNICAL RISK ANALYSIS**

|  |  |  |  |
| --- | --- | --- | --- |
| **REFERENCE:** 294380 | | | **TIS AGENCY:** CPV ARABIA |
| **TECHNICAL/S RESPONSIBLE/S:**  **DESIGN:** Mai Magdy  **SITE INSPECTIONS:** Ahmed Mansour (CIVIL ENGINEERING) | | | |
| **REVISION:**  0 | **CONTACT:**  Mahmoud Elmasry. | | |
| **DATE OF ISSUE:**  04-Aug-2024 | **FAX:** | **PHONE:** 00966553304612 | **EMAIL:** [mmasry@cpvarabia.com](mailto:mmubark@cpvarabia.com) |

**TITLE I**

|  |
| --- |
| **PRINCIPAL/OWNER:** ﺍﺣﻤﺪ ﺑﻦ ﺳﻌﺪ ﺑﻦ ﻋﺒﺪﺍﻟﻠﻪ ﺍﻟﻤﻐﺮﺑﻲ  **PROPOSER (IF DIFFERENT):** ﻣﺆﺳﺴﺔ ﺗﻌﻤﻴﺮ ﻫﺠﺮ ﻟﻠﻤﻘﺎﻭﻻﺕ**.**  **PROJECT TITLE:** ﻣﺒﻨﻰ ﺳﻜﻨﻰ  **ADDRESS:** ﺍﻟﺤﺰﺍﻡ ﺍﻻﺧﻀﺮ\_ﺍﻟﻬﻔﻮﻑ\_ﺍﻻﺣﺴﺎﺀ.  **PROPOSED USE/OCCUPATION:** المباني السكنية.  **NUMBER OF BUILDINGS:** |
| **SCOPE OF MISSION:**  **DESIGN**  **DESIGN + SITE INSPECTIONS**  **- Date of TIS involvement:** 04-Aug-2024   * **Inspections from the commencement of Works**   **YES**  **NO** * **Missions:**   **S**  **W.1**  **E**  **W.2**   **Q**  **W.3 X, specify:**  **S:** Solidity and stability, including the envelope elements  **W.x:** Waterproofing (**1**- Roofs, **2**- Façades, **3**-Basements)  **E:** Existing structures  **Q:** Works already started  **X:** Other  The TIS controls, inspections and checks marked with an X above are based on as analysis of the project, according to the requirements of the demander. |

|  |
| --- |
| **PARTIES INVOLVED**  **(Full name + Address)**  **DESIGN:** |
| * **ARCHITECT:** ﺷﺮﻛﺔ ﺍﻻﺑﺪﺍﻉ ﺍﻟﻤﻌﻤﺎﺭﻱ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **STRUCTURAL DESIGNER:** ﺷﺮﻛﺔ ﺍﻻﺑﺪﺍﻉ ﺍﻟﻤﻌﻤﺎﺭﻱ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **SOIL REPORT:** مكتب الأحساء لفحص الخرسانة والتربة والأساسات   **CONSTRUCTION:** |
| * **MAIN CONTRACTOR:** ﻣﺆﺳﺴﺔ ﺗﻌﻤﻴﺮ ﻫﺠﺮ ﻟﻠﻤﻘﺎﻭﻻﺕ * **SUBCONTRACTORS:** * **PROJECT SUPERVISOR:** ﺷﺮﻛﺔ ﺍﻻﺑﺪﺍﻉ ﺍﻟﻤﻌﻤﺎﺭﻱ ﻟﻼﺳﺘﺸﺎﺭﺍﺕ ﺍﻟﻬﻨﺪﺳﻴﺔ * **QUALITY TESTING FIRMS:** * **OTHER (SPECIFY):**   **COMMENTS ON REFERENCES OF ARCHITECTS, ENGINEERING CONSULTANTS AND CONTRACTORS OF THE OPERATION, PURPOSE OF THE INSPECTION, IF ANY:** NO REFERENCES AVAILABLE |
| **DOCUMENTS USED IN THIS REPORT**   * STRUCTURAL DRAWINGS. * ARCHITECTURAL DRAWINGS. * BILLS OF QUANTITY. * SOIL INVESTIGATION REPORT. * PROPOSAL FORM FOR INHERENT DEFECT INSURANCE.   Is there any other document or information missing which is needed for the completion of this report?  **YES**   **NO**  If YES, please specify:  - Construction schedule - Façade details - Ground slope % - Quality assurance procedures - Method statement |

**CODE TABLE**

|  |  |  |  |
| --- | --- | --- | --- |
| **NATURE OF WORKS** | **SOIL RISKS** | **STRUCTURE TYPE** | **SPECIFICATIONS** |
| **CODE N°1: CONSTRUCTION TYPE**  **A**  DETACHED OR SEMI-DETACHED  HOUSES UP TO GF+2 AND B-1  **B**  TERRACED HOUSES UP TO GF+3 AND B-1  **C1**  RESIDENTIAL BUILDINGS FROM  GF+4 TO GF+14 AND UP TO B-2  **C2**  RESIDENTIAL BUILDINGS FROM  GF+15 AND/OR FROM B-3  **D1**  OFFICES, HOTELS, SCHOOLS  **D2**  HOSPITALS, CLINICS  **D3**  COMMERCIAL BUILDINGS, RESTAURANTS, SHOPPING MALLS  **E1**  OTHER  PUBLIC BUILDINGS: THEATERS, RELIGIOUS  BUILDINGS, STATIONS  **E2**  STADES  **F1**  COMMON INDUSTRIAL  BUILDINGS, FACTORIES  **F2**  LOGISTIC PLATFORMS  **G1**  RESERVOIRS  **G2**  SPECIAL INDUSTRIAL  BUILDINGS, SMOKESTACKS,  TANKS, RETAINING WALLS, ETC  **H**  BRIDGES, FOOTBRIDGES,  JUNCTIONS AND OTHER WORKS | **CODE N°2: SLOPE**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | 0 | 1 | 2 | 3 | 4 | | <5% | 5 to 10% | 10% to 20% | 20 to 30% | >30% |   **CODE N°3: GROUND WATER AND AGRESSIVENESS**   |  |  | | --- | --- | | 0 | no water table | | 3 | works below water table | | 4 | works above water table |  |  |  | | --- | --- | | N | non-aggressive water or soil | | Y | aggressive water or soil |   **CODE N°4: FOUNDATIONS**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | A | footings | | | | | | B | raft | | | | | | final settlement | 0 | 1 | 2 | 3 | 4 | | <2 cm | 2 to 5 cm | >5 cm |  |  | | C | piles or contiguous piles wall | | | | | | D | friction piles | | | | | | E | diaphragm wall | | | | | | F | shafts | | | | | | depth | 0 | 1 | 2 | 3 | 4 | | 0 to 3 m | 3 to 10 m | 10 to 25 m | 25 to 30 m | >30 m | | Z | Other foundation type | | | | |   **CODE N°5: GROUND SPECIFIC RISKS**   |  |  | | --- | --- | | O | no ground specific risks | | P | underground quarries, sinkholes, karsts | | Q | mining ground | | R | Anchored earth retaining structure.  (h > 3 meters) | | S | underpinning, basement construction | | T | ground consolidation (grouting compaction; dynamic compaction/vibration) | | U | hazardous storage, concentrated surcharge loads, embankment | | V | Compressive layer | | W | founding on fill | | X | other ground risk | | Y | at least 2 ground specific risk | | Z | new foundation type | | CODE N°6: STRUCTURE  A  VERTICAL STRUCTURES MASONRY  B  REINFORCED CONCRETE CAST IN-SITU  **C**  PRECAST REINFORCED CONCRETE - PREFABRICATED IN FACTORY RESIDENTIAL BUILDINGS FROM  GF+4 TO GF+14 AND UP TO B-2  **D**  PRECAST REINFORCED CONCRETE - ON SITE  **E**  PRESTRESSED CONCRETE EXCL. POST-TENSIONED CONCRETE  **F**  STEEL WORKS - SITE ASSEMBLY  **G**  PRE-ASSEMBLED STEEL WORKS  **H**  ON SITE WELDING  **I**  TIMBER STRUCTURE  **X**  TRADITIONAL COMPOSITE STRUCTURE  **Y**  WORKS ON EXISTING STRUCTURES - BASEMENT CONSTRUCTION - NEW FLOORS  **Z**  NEW STRUCTURAL SYSTEMS INCL. POST-TENSIONING | **CODE N°7: FACADE**   |  |  | | --- | --- | | A | concrete wall or masonry | | B | sandwich or timber panels | | C | curtain walls – steel frame glazing | | D | curtain walls – glazing fixed with glue | | E | curtain walls – glazing fixed bolts | | F | breathable glazed curtain wall | | G | cable curtain wall | | Z | other type |   **CODE N°8: HEIGHT**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Height - Ho | <25m | 25 to 35m | 35 to  60m | 60 to 100m | >100m | | Maximum Headroom - Hp | <8m | 8 to 15m | 15 to  35 m | 35 to 50m | >50m |   **CODE N°9: DEPTH**   |  |  |  |  |  | | --- | --- | --- | --- | --- | |  | 1 | 2 | 3 | 4 | | Depth | <5m | 5 to 10m | 10 to 15m | >15m |   **CODE N°10: SPANS**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Spans | <15m | 15 to 20m | 20 to 30m | 30 to 40m | >40m | | Spans (timber) | <10m |  |  |  | >10m |   **CODE N°11: CANTILEVER**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | |  | 0 | 1 | 2 | 3 | 4 | | Cantilever | None | 0 to 2m | 2 to 5m | 5 to 10m | >10m |   **CODE N°12: SITE EXPOSED**   |  |  |  | | --- | --- | --- | |  | 0 | 1 | | Distance to the sea | >5km | <5km |   **CODE N°13: WND SENSITIVITY**   |  |  | | --- | --- | | 0 | Concrete or masonry structure | | 1 | Steel, timber or composite structure |   **CODE N°14: WATERPROOFING OF ROOFS**   |  |  | | --- | --- | | A1 | pitched roof - tiles | | A2 | pitched roof - steel roof-deck | | A3 | pitched roof - sandwich panels | | B1 | flat roof-non practicable normal waterproofing | | B2 | flat roof-non practicable inverted waterproofing | | B3 | flat roof-practicable normal waterproofing | | B4 | flat roof-practicable inverted waterproofing |   **CODE N°15: WATERPROOFING OF BASEMENT**   |  |  | | --- | --- | | A | External treatment (PVC, bitumen based,  polyurethane membranes) | | B | Crystallization technology by concrete additive | | C | Other | | Z | No basement | |

**PROJECT OVERALL VIEW**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CODE** | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **10** | **11** | **12** | **13** | **14** | **15** |
| **BUILD.1** | NA | 0 | 0 N | 0 | O |  | NA | 0 0 | 1 | 0 | 0 | 0 | 0 |  | Z |
| **Concerning the code table above, please complete one line per building/structure and explain each code below. PLEASE EXPLAIN IF SEVERAL CODES INDICATED IN THE SAME CASE.**  CODE 1: NA  CODE 2: No value has been indicated in the geotechnical report, so it is estimated that due to the geology of the area it is less than 5%.  CODE 3: Ground water level was not detected in the boreholes. Non-aggressive due to water or soil ( Chloride in Soil= % , Sulfate in Soil= % )  CODE 4: The foundation type: and the settlement value: mm  CODE 5: No Ground Specific Risks  CODE 6:  CODE 7: NA  CODE 8: The total height is: m and the maximum headroom (Hp):m  CODE 9: Level of Foundation from street level: m  CODE 10: The maximum span is, approximately: m  CODE 11: No Cantilevers have been founded in the floor slabs  CODE 12: The distance to the sea > 5 km  CODE 13: Concrete or masonry structure  CODE 14: The roof waterproofing is not mentioned and the common case is  CODE 15: No basement  **Summary description of the work, nature of the foundations and of the structure, specify the particularities (for example the presence of a ground water level and its position in relation to the last basement, the presence of basements or existing buildings along an excavation).**  NA, Total Building height = m  The project consists of reinforced concrete beams and columns, founded on | | | | | | | | | | | | | | | |

|  |
| --- |
| **DRAWINGS**  **Please annex the following drawings, if available:**  **LOCATION**  **GENERAL DRAWING**  **PLANS**  **SECTIONS**  **FACADES & ROOFS & TERRACES**  **FOUNDATIONS**  **OTHER, PLEASE SPECIFY:**  THESE DRAWINGS ARE ATTACHED IN ANNEX I. DRAWINGS. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **PROVISIONAL TOTAL COST OF WORKS**     |  |  | | --- | --- | | Are Architect and Engineering Consultants fees included in the cost of the works: | YES  NO |  1. Total cost of the works: 753,250.00 SAR 2. Structural works: 450,000.00 SAR 3. Envelope: 50,000.00 SAR 4. Non-structural works: 70,000.00 SAR 5. Equipment, fixtures, and fittings: 20,000.00 SAR 6. External works: 50,000.00 SAR 7. Design and professional fees: 15,000.00 SAR 8. Taxes: 98,250.00 SAR  |  |  | | --- | --- | | Is there any special equipment (industrial machinery used in the manufacture of products or services) included in the cost other than those usually used in common constructions? | YES  NO |   If so, please specify: Nature:  Cost:  **DATES AND CONSTRUCTION TIMES**  Expected duration of work (months): 12months  Date of commencement of construction: 31-Jul-2024  Date of the first on-site visit of the Inspection Agency: 15-Aug-2024  Expected date of practical completion: 30-Jul-2025 |

**TITLE II**

|  |
| --- |
| **SITE DESCRIPTION**  Is the building likely to be flooded (river, lake or sea, ground water level)?  YES  NO  Maximal level of the ground water level to ground floor and to the last basement:  - Ground water level was not detected in the boreholes  - Ground floor level is +0.3 m.  - No Basement    Is there a system to prevent the effect of the water under-pressure? NA  YES  NO  If YES, please specify:  Is the building located in a seismic area? Region 2 YES  NO  If YES, could you specify the level of protection? (Specify: statutory or contractual?): statutory  Acceleration value: PGA=Not Mentioned .  Indicate in % the ground slope: No value has been indicated in the geotechnical report, so it is estimated that due to the geology of the area it is less than 5%..  If >15%, was the landslide risk evaluated in the Geotechnical Report and/or the design? NA  YES  NO  If NO, please make a reserve in conclusions.  Is the building located in a cyclone area?  YES  NO  Wind speed considered in the calculations (km/h): approximately 152 km/h  Is snow load applicable?  YES  NO  If so, snow load value:  Is the site located in a hostile environment (<5 km sea, soil, and underground water)?  YES  NO  If YES, specify the nature and the protection provided: |

|  |
| --- |
| **GEOLOGY - TOPOGRAPHY – FOUNDATIONS**  Has a geotechnical engineer been involved in the design?  YES  NO  Is there a geotechnical report?  YES  NO  (If YES, please indicate the scope, number, and type of geotechnical tests and describe the layers including thickness).  Number of boreholes:  - Borehole 1: BH-1, depth of: m  Type of tests and trials:  - Chemical Analysis |

|  |
| --- |
| Are the adopted foundations founded on natural soil?  YES  NO  Depth of excavation: m from the street level.  Depth of soil supporting foundations: m from the street level.  Nature of soil supporting foundations:  All earthworks to be performed shall be compliant with the recommendations indicated in the geotechnical report.  Please describe the foundations (level of foundation, bearing capacity, bearing pressure):   * Foundation type: * Bearing Capacity: kg/cm2.   Are the conclusions of the Geotechnical Report relevant?  YES  NO  If NOT, please explain the reason:  Is the ultimate settlement indicated in the geotechnical report?  YES  NO  Please indicate the value: mm.  Is the foundation system in line with the soil report?  YES  NO  If NOT, please precise the differences and the reason:  Has the RD1 report been filled in?  YES  NO  If YES, please mark below the reason:  Presence of back fill or compressible or expansible layers being used as foundations for the works  Presence of piles, diaphragm walls or shafts superior to 3 m deep  Presence of ground slopes exceeding 30% or cliffs sides  Risk of ground sliding after soils excavation  Are additional surveys needed?  YES  NO  If YES, please precise:  - According to 303 Structural - Soil and Foundations Standard, in table 2.1, the minimum depth of one third of the boreholes for this case is 6 m (measured from level of foundation bottom), and this does not comply. - According to 303 Structural - Soil and Foundations Standard, in table 2.1, the minimum depth of two thirds of the boreholes for this case is 4 m (measured from level of foundation bottom). This does not comply.  - According to 303 Structural - Soil and Foundations standard, in table 2.1, the minimum number of boreholes must be three at least, and this doesn’t comply. - Shear Test Parameters - Soil/Rock Quality Degree Test |

**TITLE III**

|  |
| --- |
| **The items below must be descripted briefly but detailed enough to include any relevant information.**  The used technologies must be specified where is possible: traditional construction, prefabricated structural elements, steel/concrete mixed structures, pre-tensioned (factory or site), welding (factory or site), etc  It is a traditional system.  **Please indicate if innovative materials or technics are used which means (completion of RD2 report mandatory).**  No innovative materials or technics are used.  **VERTICAL STRUCTURES**  Full description of the adopted model.    Are there non-vertical loads/transfer structures?  YES  NO  **VERTICAL ELEMENTS (COLUMNS, BEARING WALLS)**  **Nature (reinforced or prestressed concrete, metal, timber...):**  **HORIZONTAL STRUCTURAL ELEMENTS**  **FOUNDATIONS**  **Nature (concrete, masonry, ..):** .  **Footings**  fc`: Not Mentioned  Fy: Not Mentioned  **FLOOR SLABS**  **Nature (reinforced or prestressed concrete, metal, timber...):**  **ROOF STRUCTURAL ELEMENTS**  Please note if those are:  FLAT  PITCHED  If flat, similar to floor slab?  YES  NO  If NO indicate modifications:  If pitched, please note its main characteristics: |

|  |
| --- |
| HEAVY FACADES  Type, total thickness, rendering, cladding...  (Specify load-bearing facades or not, precast, or not.)  **Façade details:**  NA  **LIGHT-WEIGHT FACADES**  Not Applicable  Frame (aluminum, steel, timber or other):  Filling (glass, composite wall, in this case, specify the constitution):  Total surface of each type of façade:  Possibility to replace the façade elements easily:  YES  NO  **HORIZONTAL STABILITY**  Traditional structural elements (frame, inner walls, bracings...)?  YES  NO  If not: fill in the complementary report RD2  Traditional structural elements are reinforced concrete frames.  **BASEMENT WATERPROOFING**  The project doesn´t include basement  Presence of water (water flow, water table)?  YES  NO  If YES: solution chosen (waterproofness, drainage, and shaft lining...)  waterproofing system:  **FACADE WATERPROOFING** |

|  |  |
| --- | --- |
| ROOF WATERPROOFING  **Roof details:**  The roof details are not mentioned.   |  | | --- | |  | |
| GROUND SLAB  Is the ground slab suspended?  YES  NO  If NOT, is the ground slab bearing on backfill?  YES  NO  Maximum thickness of backfill: 0.1 m from the bottom of the foundation to the bottom of the slab on grade.  Loads:  Spread:  YES  NO Value: not informed  Concentrating/rolling:  YES  NO Value:  Other:  YES  NO Value: |

**TITLE IV**

|  |
| --- |
| **IDENTIFIED AGGRAVATING RISKS AND ADDITIONAL INFORMATION:**  (For example, large span beams or slabs, foundation for heavy and/or vibrating machinery, etc.)  It is necessary to submit the documents indicated in title I, referring to the documents used in this report.  **Design (RD5):**  - The soil classification and site investigation have not been conducted in compliance with SBC 303-2018 (Ch. 2, Sec. 2.3 & 2.4) and SBC 1101 (Sec. 704).  Please Conduct a new soil investigation in accordance with SBC 303-2018 and SBC 1101 requirements, update the project design based on the new findings, Please send us the updates once completed. - The foundation reinforcement ratio does not comply with SBC 1101, Sections 707.10.1.1, 707.10.1.2, 707.10.2, 709.1.7, and 707.10.  testttttttt - The settlement mentioned in the geotechnical report does not comply with SBC 1101, Section 706, and SBC 303, Section 8.5  Review the settlement mentioned in the geotechnical report to ensure compliance with SBC 1101, Section 706, and SBC 303, Section 8.5, and update the report accordingly. - The structural model does not comply with the design requirements for bending moment, shear, immediate deflection, and long-term deflection as stated in SBC 1101, Sections 4B5, 4B11, 4C3.1 to 4C3.4.1.3, and Tables 4C-1 and 4C-2.  Review the structural model to ensure compliance with design requirements for bending moment, shear, immediate deflection, and long-term deflection as stated in SBC 1101, Sections 4B5, 4B11, 4C3.1 to 4C3.4.1.3, and Tables 4C-1 and 4C-2, and make necessary adjustments. - Openings and embedded conduits and pipes in structural members are not done in accordance with SBC 1101, Section 7A8.  Review and modify the design of openings and embedded conduits and pipes in structural members to ensure compliance with SBC 1101, Section 7A8, and implement necessary changes.  **Inspection (RD5):**  - The Foundations are supported on backfill layers more than 30cm. - The soil contains some aggressive items ( Chloride in Soil= 0.171 % Sulfate in Soil= 0.119 % ) and the design concrete compressive strength is22 MPa. which isn`t enough to resist this soil aggressiveness, and it should be at least 31 MPa. (The inspection team will check at the site) - The location of the (water tank/ Septic tank) was not specified on the plans. It must be considered that the location of the tank near the building affects the stability of the building’s foundations and exposes the structure to risk. - The site investigation and report have not been expanded to include property boundaries, grading dimensions, drainage plans, building locations, and the impact of geological conditions as per SBC 303, Section 3.1. - The minimum mat thickness has not been calculated based on punching shear and diagonal-tension shear according to SBC 303, Section 8.9.3.2, including investigations for columns at the mat edge and perimeter load-bearing walls as specified in SBC 304, Chapter 15. - The foundation waterproofing is not in compliance with SBC 1101, Section 711, and does not ensure that the parts of the building below ground level are damp-proofed using approved waterproofing materials. - The walls or partitions constructed from adobe units do not comply with the requirements of SBC 201, Section 2109.3.4.5.1.  **Technical reservations:**  - Technical reservation: The ground slab is supported on a backfill of more than 30cm.  The contractor must execute the filling following a procedure approved by a geotechnical firm, which will oversee the monitoring too (for instance by making regular compaction tests). The TIS must be informed about the compaction procedure and check the process/results (The inspection team will check at the site). - Technical reservation: The minimum footing depth below natural ground level and the minimum concrete cover to reinforcement not comply with SBC 303, Section 5.2 and Section 5.4.2.6  Ensure footing depth and concrete cover comply with SBC 303, Section 5.2 and Section 5.4.2.6, and update the design accordingly. - Technical reservation: The concrete cover for the steel reinforcement has not been verified according to SBC 1101, Section 4A7.1.  Verify that the concrete cover for steel reinforcement complies with SBC 1101, Section 4A7.1 requirements, and adjust any non-compliant designs. - Technical reservation: The damp-proofing and waterproofing are not compliant with SBC 303, Sections 13.1-13.5, SBC 1101, Sections 711.1 to 711.2.3, Figure 7.21, and SBC 303, Chapter 13, using approved materials and specifications.  Ensure that the damp-proofing and waterproofing comply with SBC 303, Sections 13.1-13.5, SBC 1101, Sections 711.1 to 711.2.3, Figure 7.21, and SBC 303, Chapter 13, by utilizing approved materials and specifications. - Technical reservation: The minimum densities for design, design loads, and load combinations in the structural model do not comply with the requirements of SBC 301, Section 4.3, Section 4.4, Tables 3.1, 3.2, and 4.1, Chapter 11, SBC 303-2018, Chapter 2.6, SBC 301, Section 1.5, Section 2.3, and Section 2.4.  Revise the structural model to ensure compliance with the requirements of SBC 301, including the minimum design densities, loads, and load combinations as specified in Sections 4.3, 4.4, Tables 3.1, 3.2, 4.1, Chapter 11, SBC 303-2018, Chapter 2.6, and Sections 1.5, 2.3, and 2.4.  **Notes:**  - Structural analysis report should be provided. - The warranty of facades insulation must be provided by the client before issuing (RD3). - Project located in a seismic zone (PGA is in-between 0.04-0.10g); A seismic calculation must be provided in these cases. - The soil report does not justify the use of soil parameters for calculating bearing capacity according to SBC 1101, Section 705, nor does it confirm that the contact design bearing capacity is equal to or less than the soil bearing capacity as per SBC 303, Section 8.9.3.1 and Section 4(B). - The longitudinal bars and ties for columns do not comply with SBC 1101 - The additions to existing buildings do not comply with SBC 201 requirements for new construction, and the conditions for exemptions from Chapter 11 compliance as specified in Sections 1101.2, 1103.1, 1103.2, 1103.3, 1103.3.1, 1103.3.2, 1103.3.3, and 1103.3.4 have not been met. - The built-up roof covering does not comply with the material standards specified in SBC 1101, Section 905.9.2.  **Aggravating risks:**  -  -  -  - It was not specified how the connection between the masonry of the facade and the concrete structure is made. - No specification has been found regarding insulation and waterproofing of the joints between different types of facades. - There are no details about lintels (dimension and reinforcement). - The soil study doesn't present shear test parameters. - The soil study doesn't present soil/rock quality degree tests. |

|  |
| --- |
| **TECHNICAL STANDARDS USED IN THE PROJECT:**   * 301 Structural – Loading and Forces. * 302 Structural – Testing and Inspection. * 303 Structural – Soil and Foundations. * 304 Structural – Concrete Structures. * 305 Structural – Masonry Structures. * 306 Structural – Steel Structures.   Are they relevant?  YES  NO  If NOT, please specify why: |

**TITLE V**

**CONCLUSIONS**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Additional reports needed to estimate the risks and issuing date:  RD1 Special Foundation Report – Expected date:  RD2 Innovative materials/procedures report – Expected date:  RD3 Waterproofing assessment report (Waterproofing Certificate Approval) – Expected date: 30-Jul-2026  RD5 Works interruption report – Expected date: It will be issued to highlight major deviation noted on site during inspection or failure to submit the required documents  RD6 Final risk assessment report (Certificate of Approval) – Expected date: 31-Jul-2025  **RISK TECHNICAL ASSESSMENT**  (Risk assessment based on the checked documents. Please specify topics requiring special focus).  Within the scope of its mission, the CPV, based on the technical documentation received from the project and after its general preliminary analysis and reflected in this report, it is considered that the TECHNICAL RISK IS AGGRAVATED However, If the questions raised in this report are clarified, some of the aggravating situations can be reduced to a normal risk situation.  A list of AGGRAVATING RISKS is included in title IV of this document.   |  | | --- | | TI302-294380 | | TI3006-294380 | | TI3013-294380 | | TI3020-294380 | | TI3027-294380 |   technical reserves were opened: |
| Does the risk require the involvement of any TIS headquarter expert?  YES NO  If YES, specify the reason:  Minimum number of site visits: 5  Of which:  -Foundations visits: 01  -Structure visits: 02  -Waterproofing (if relevant): 01  -Final inspection: 01 |

Riyadh, 04-Aug-2024


THE TECHNICIAN/S IN CHARGE OF THE CONTROL



ENG. Mai Magdy

Civil engineer

Project Analysis Department Manager



ENG. MAHMOUD ELMASRY

Civil engineer

Quality Control Manager



ENG. Alaa Abdulkareem

Civil engineer

# ANNEX I. DRAWINGS.

|  |
| --- |
|  |
|  |

|  |
| --- |
|  |

|  |
| --- |
|  |
|  |

**LOCATION**